变更说明：因WOS节点出现一块硬盘故障，需要更换硬盘，具体步骤如下：
 
 
1. 检查/var/log/message日志，查看是否有故障硬盘。
cat /var/log/message | grep "Medium Error"
[image: 计算机生成了可选文字:
Dec 
Dec 
0 ： 0 ： 17 
Dec 
0 :0 :17 
Dec 
0 :O ； 17 
Dec 
Dec 
0 ： 0 ： 17 
Dec 
0 :0 :17 
Dec 
Dec 
Dec 
0 ： 0 ： 17 
Dec 
0 :0 :17 
Dec 
B 06 ： ： 01 
Dec 
0 ： O: 17 
Sd 0 ： 0 ： 17 
Dec 
B 05 ： 的 ： 15 swosda02 
B 05 ： 10 ： swosda02 
8 05 :10: 12 svosda02 
B 05 ： 10 ： 49 swosda02 
8 05 :10: 57 svosda02 
B 13 ： 23 ： 05 swosda02 
B 05 ： 的 ： ， S 」 日 02 ． SZZb 
8 05 ： 的 ： 23 svosda02-szzb 
B 05 ； 的 ； 42 swosda02-szzb 
B 05 ： 的 ： 57 ， sda02 ． SZZb 
B 05 :10 ； 19 swosda02-szzb 
B 05 ： 10: 42 ， Sda02 ． SZZb 
B 05 :12 ； 16 svosda02-szzb 
swosda02-szzb 
-szzb 
-szzb 
-szzb 
-szzb 
-szzb 
-szzb 
kernel: 
kernel: Sd 
kernel: Sd 
kernel: 
kernel: 
kernel: Sd 
kernel: Sd 
kernel: 
kernel: 
kernel: Sd 
kernel: Sd 
kernel: 
kernel: Sd 0 ： 0 ： 17 ： 0 ： 
Sd 
kernel: Sd 0 ： O: 17 ： 0 ： 
Sd 
Sd 
Sd 
Sd 
0 :O ； 17 ； 
0 ： O: 17 ： 
0 :O ； 17 ： 
Isdpl 
Isdpl 
Isdpl 
tsdpl 
tsdpl 
Isdpl 
Isdp ] 
Isdpl 
Isdpl 
Isdpl 
Isdpl 
Isdpl 
tsdpl 
Isdpl 
Sense 
Sense 
Sense 
Sense 
Sense 
Sense 
Sense 
Sense 
Sense 
Sense 
Sense 
Sense 
Sense 
Sense 
Key 
Key 
Key 
Key 
Key 
Key 
Key 
Key 
Key 
Key 
Key 
Key 
Key 
Key 
Medium 
Medlum 
№ dlum 
№ dium 
№ dlum 
Medlum 
№ dium 
№ dium 
№ dium 
Medlum 
№ dlum 
№ dium 
№ dium 
Medlum 
Erro r 
r 
Erro r 
Erro r 
Erro r 
r 
r 
Erro r 
Erro r 
r 
r 
Erro r 
Erro r 
r 
(current 1 
(currentl 
{ currentl 
(currentl 
(current 1 
(currentl 
{ current 1 
(current 1 
(current 1 
(currentl 
(current ] 
(currentl 
(current 1 
(currentl 
(descriptor) 
(descriptorl 
(descriptorl 
(descriptor) 
(descriptor) 
(descriptorl 
(descriptorl 
(descriptor) 
(descriptor) 
(descriptorl 
(descriptorl 
(descriptorl 
(descriptor) 
(descriptorl 
” 0t 、 vosda02 ． SZ 外 司 ， cat /var/log/nessages | 
grep Medium' ]
sdp有磁盘告警错误。
 
1. 查看该硬盘序列号。
[image: ]
 
WOS后台查看磁盘信息。
[image: 计算机生成了可选文字:
swosda02- 
SZZb 
0 1 23E 
Manufacturer 
A02 
3 
A04 
A05 
A06 
7 
A08 
A09 
A10 
A12 
A13 
A14 
A15 
shahe2 
Model 
Active 
1 巳 2M 
63959 
51 日 21 
81 
• Drives 
引 Ot 旧 
2 
3 
4 
5 
6 
7 
8 
1 2 
1 3 
1 
1 5 
1 6 
． Details 
Enclosure 旧 
Status 
Active 
的 e 
舡 的 e 
Active 
Active 
的 e 
舡 的 e 
Active 
Active 
的 e 
舡 的 e 
Active 
Active 
的 e 
舡 的 e 
Active 
Serial Number 
2011P6 
ZCIIPEMZ 
ZC11P6BO 
ZCIIN 、 'R6 
2011P6J3 
z011mP0 
ZCII PE × 0 
ZCII PE × 2 
2011 P521 
z011 LPY6 
ZC11P61V 
ZC1070CV 
2011P6JH 
z011N 、 ' RI 
ZC 11 PATS 
之 c11 PB4C 
Capacitf 
00TB 
4 00TB 
# 00TB 
# 00TB 
00TB 
4.00TB 
4 00TB 
# 00TB 
00TB 
4.00TB 
4 00TB 
# 00TB 
00TB 
4.00TB 
# 00TB 
# 00TB 
ST O NM 35 豳 1 07 
ST40 NM 35 ． 1v41 07 
ST40 NM 35 ． 1v41 07 
ST # 0 NM 35 ． 1 1 07 
ST O NM 35 豳 1 07 
ST40 NM 35 ． 1v41 07 
ST40 NM 35 ． 1v41 07 
ST # 0 NM 35 ． 1 1 07 
ST O NM 35 豳 1 07 
ST40 NM 35 ． 1v41 07 
ST40 NM 35 ． 1v41 07 
ST # 0 NM 35 ． 1 1 07 
ST O NM 35 豳 1 07 
ST40 NM 35 ． 1v41 07 
ST40 NM 35 ． 1v41 07 
ST # 0 NM 35 ． IV # 1 07 
FAKE ENCLOSURE 
v2 工 O 」 .0_ggcecacg 
Software Version ]
A16 对应 woscore-disk16
[image: 计算机生成了可选文字:
Irooteswosda02-szzb 、 11 /dev/woscore-disk* 
root 3 北 1 
。 1 
- ， sdk 
r 、 
1 ， r 、 
1 
1 r 、 { r•WX 
r 、 
1 ， r 、 
1 ， 
1 r 、 r•WX 
1 r•WK 
1 ， r 、 
1 
1 r 、 { r•WX 
1 r•WK 
1 r 只 
1 
1 
1 
1 
1 
1 
1 
1 
1 
1 
1 
1 
1 
1 
1 
1 
1 
root 
root 
root 
root 
root 
root 
root 
root 
root 
root 
root 
root 
root 
root 
root 
root 
root 3 北 1 
root 3 北 1 
root 3 北 1 
root 3 北 1 
root 3 北 1 
root 3 北 1 
root 3 北 1 
root 3 北 1 
root 3 北 1 
root 3 北 1 
root 3 北 1 
root 3 北 1 
root 3 北 1 
root 3 北 1 
root 3 北 1 
1 
1 
1 
1 
1 
1 
1 
1 
1 
1 
1 
1 
1 
1 
1 
1 
m19 /dev/woscore-disk01 ． ， sda 
2 丑 9 /dev/woscore-disk02 - ， sdb 
19 /dev/woscore-disk03 - ， （ 
团 19 /dev/woscore-disk04 · ， sdd 
m19 /dev/woscore-disk05 sde 
m19 /dev/woscore-disk06 ． ， sdf 
2019 /dev/woscore-disk07 
团 19 /dev/woscore-diskog · ， sdh 
m19 /dev/woscore-disk09 sdi 
2 丑 9 /dev/woscore-disk10 
2019 /dev/woscore-diskll 
团 19 /dev/woscore-disk12 一 ， sdl 
m19 /dev/woscore-disk13 、 d 
m19 /dev/woscore-disk14 ． ， sdn 
2010 /dev/woscore-disk16 ． ， Sdp 
Iroot@swosda02-szzb 司 ， 日 ]
 
记录当前盘符顺序和接口位置，避免重启后出现盘符接口位置错乱，SCSI设备数量为20个。
[image: 计算机生成了可选文字:
(rootes 、 iosda02-szzb 司 ， 
brv-r 、 
． 1 
． 1 
16 Dec 
一 1 
32 Dec 
一 1 
48 Dec 
brv-rw- 
． 1 
64 Dec 
． 1 
日 0 Dec 
· 1 
96 Dec 
一 1 
112 Dec 
brv-r 、 
． 1 
128 Dec 
． 1 
14 Dec 
一 1 
160 Dec 
8 15 ： 14 /dev/sdl 
一 1 
176 Dec 
brv-r 、 
． 1 
192 Dec 
． 1 
208 Dec 
一 1 
22 Dec 
一 1 
240 Dec 
brv-r 、 
． 1 
． 1 
一 1 
一 1 
/sd* 
0 Dec 
0 Jul 
1 北 1 
ul 
2 
3 〕 ul 
/sd* 
1 
1 
1 
1 
-rv- 
-rv- 
root 
root 
root 
root 
root 
root 
root 
root 
root 
root 
root 
root 
root 
root 
root 
root 
root 
root 
root 
root 
disk 
巳 
disk 
巳 
dlSk 
巳 
dusk 
巳 
disk 
巳 
disk 
巳 
dlSk 
巳 
dusk 
巳 
disk 
巳 
disk 
巳 
disk 
巳 
dusk 
巳 
disk 
巳 
disk 
巳 
dlSk 
巳 
dusk 
disk 6 ， 
disk 6 ， 
dlSk 65 丿 
dusk 65 丿 
8 15 ： 14 /dev/sda 
日 巧 ： 15 /dev/sdb 
15 ： 14 /dev/sdc 
8 15 ： 14 /dev/sdd 
8 15 ： 15 /dev/sde 
日 15 ： 14 /dev/sdf 
． 15 /dev/sdg 
e 15 ． 
8 15 ： 15 /dev/sdh 
8 15 ： 14 /dev/sdi 
' 14 /dev/sdj 
日 15 ， 
15 ： 14 /dev/sdk 
8 15 ： 14 /dev/sdn 
日 15 ： 14 /dev/sdn 
e 15 ： 14 /dev/sdo 
· 14 /dev/sdp 
8 15 ． 
/dev/sdq 
2019 /dev/sdql 
/dev/sdq2 
/dev/sdq3 
2019 
2010 
2010 
(rootesvosda02-szzb 司 
20 
(rooteswosda02-szzb 司 # ]
 
1. 从WOS中移除磁盘woscore-disk16 UDEV
vi /etc/udev/rules.d/99-woscore-sw-disks.rules
注释如下行
[image: 计算机生成了可选文字:
sd* ' 
KERNEL—" Sd* " 
SYMLINK+z"WOSCOre 
SYMLINK+—"WOSCOre 
sd* ' 
SYMLINK+z"WOSCOre 
KERNEL—" Sd* " 
SYMLINK+—"WOSCOre 
sd* ' 
z/dev/$name", RESULT—" 3 ， 500a2g502e5 " 
KERNEL—" Sd* " 
KERNEL—" Sd* " 
RESULT—" 35000c 
sd* ' 
350e0c 
KENSJEL—" Sd* " 
KERNEL—" Sd* " 
(rootesvosda02-szzb 司 ， cat /etc/udev/rules.d/99-woscore-sw 
-disks rules 
--whltehsted 
--whltehsted 
--whitelisted 
--whltehsted 
--whltelusted 
--whitelisted 
--whltehsted 
--whltehsted 
--whitelisted 
--whltehsted 
--whltehsted 
--whitelisted 
· replace-whitespace 
replace-whitespace 
- replace-whitespace 
- replace-whltespace 
· replace-whitespace 
replace-whitespace 
- replace-whitespace 
- replace-whitespace 
· replace-whitespace 
replace-whitespace 
- replace-whitespace 
- replace-whltespace 
replace-whitespace 
- replace-whitespace 
- replace-whltespace 
-deuce 
-/dev/$name" 
-deuce 
z/dev/$name" 
-device 
E/dev/$name" 
-device 
-/dev/$name" 
-deuce 
-/dev/$name" 
-deuce 
Z/dev/$name" 
-device 
r/dev/$name" 
-device— 
/dev/$name" 
-deuce 
-/dev/$name" 
-deuce 
-device 
嬲 惹 
-device 
-deuce-/dev/$ 
-deuce-/dev/$name 
-device-/dev/$name" 
-device-/dev/$name" 
35000c Oa 5B 酽 
RESULTz:" 3 ， 0c500a2g5 c 酽 
RESULT—" 3 ， 0c500a295ae3b " 
RESULT—" 35000c500a29592f0 
RESI 35C Oc 0a2g5 5 
RESULTÆ' 3 ， 500a2g6 3 
RESULT—" 3 ， 0c500a295d493 " 
RESULT—" 35000c 0a295e b " 
RESI 35000c500a 凶 Scaf 
RESULT—" 3 ， 0c500a295bfe 酽 
3 ， 500a2g5a31 酽 
“ 3 ， 0c500a296B 丿 de " 
RESULT—— ' 3 000500 29m 5 " 
SYMLIFIK+—" 
WO SC 0 re 
ML + 酽 
WO SC 0 re 
SY 、 L 巋 + 
WO SC 0 re 
SYMLINK+Z" 
WO SC 0 re 
SY 、 L 巋 + 
WO SC 0 re 
MLI 卜 粼 + 
WO SC 0 re 
*141 + = 
"woscore 
． dl 酞 01 " 
． di 酞 02 " 
-disk03" 
-disk04" 
． di 0 宁 
豳 i 酞 06 " 
-disk07" 
-disk08" 
． di 0 酽 
． di 酞 1 俨 
-diskll" 
-disk12" 
-disk13" 
． di 酞 1 酽 
-disk15" 
ATTRIqueue/schedulerF"dead11ne' 
ATTRIqueue/scheduleNz"deadline" 
ATTRIqueue/scheduler)-"deadline" 
ATTRIqueue/scheduler)-"dead1ine' 
ATTRIqueue/scheduler)-"deadline' 
ATTRIqueue/scheduleNz"deadline" 
ATTRIqueue/schedulerF"deadline" 
ATTRIqueue/scheduler)-"dead1ine' 
ATTRIqueue/scheduler)-"dead1ine' 
ATTRIqueue/scheduler)z"deadline" 
ATTRIqueue/scheduler)-"deadline" 
ATTRIqueue/scheduler)-"dead1ine' 
ATTRIqueue/scheduler)-"dead1ine' 
ATTRIqueue/scheduleNz"deadline" 
ATTRIqueue/schedulerF"deadline" 
SUBSYSTEM——"b10ck" 
sd*' 丿 SUB ， T 日 繼 b10 酞 “ 
SUBSYSTEM——"blOCk" 
KERNEL—" Sd* " ， Sl 」 BSYSTEM——"blOCk" 
SLIB ST 繼 b10 醵 “ 
sd* SUB ST 卧 忙 b10 酞 “ 
KERNEL—" Sd* SUBSYSTEM——"blOCk" 
Sl 」 BSYSTEM——"blOCk" 
9 」 B ST 繼 b10 醵 “ 
sd*' 丿 馴 B ST 日 繼 b10 酞 “ 
SUBSYSTEM——"blOCk" 
Sl 」 BSYSTEM——"blOCk" 
SUBSYSTEM——"b10ck" 
sd*' 丿 SUB ST 日 繼 b10 酞 “ 
SUBSYSTEM——"blOCk" 
Sl 」 BSYSTEM——"blOCk" 
PROGRAM—" /sbin/scsl id 
PRO 、 一 “ /sbin/scsl id 
PR 、 = = " /sbin/scsi id 
PRO 田 1 一 " /sbin/scsi id --whitelisted 
PROGRAM—" /sbin/scsl id 
PROGRAM—"/sbin/SCS1 id 
PROGRAM—" /sbin/scsi id 
PRO 田 1 = = " /sbin/scsi id --whitelisted 
F 0 M 一 “ /sbin/scsl id 
PRO 、 一 “ /sbin/scsl id 
PROGRAM—" /sbin/scsi id 
PROGRAM—" /sbin/scsi id --whitelisted 
PROGRAM—" /sbin/scsl id 
PRO 、 一 “ /sbin/scsl id 
PROGRAM—" /sbin/scsi id 
PRO 田 1 = = " /sbin/scsi id --whitelisted 
/ oscore 
+ 一 0 SC 0 re 
NK+z"woscore 
， SYML 
"woscore 
SYMLINK+—"woscore-diSk16" ]
 
1. 重新检索SCSI标识符
start_udev
[image: 计算机生成了可选文字:
root3swosda01-szzb ， start—udev 
starting udev ： 
trootOswosda01—szzb 司 ， ]
 
1. 登录WOS后台查看16号盘状态从active变成Down后，服务器重启。
 
1. 系统重启时不要进系统，先进入IDRAC管理控制台重置密码，再重启进入系统，检查IDRAC是否可以正常登录，根据SN查看故障盘盘位并记录，然后关机。
 
1. 打开机箱更换硬盘。
 
1. [bookmark: _GoBack]登录IDRAC，找到RAID卡管理页面，找到刚刚更换的盘位，修改配置为“转换为非RAID”，并立即应用。
[image: 计算机生成了可选文字:
]
 
1. 查看新增盘符是否识别到，设备数量是否为20个。
 
1. 查看新盘的scsi id 记录下来，并在/etc/udev/rules.d/99-woscore-sw-disks.rules中进行修改。
scsi_id --device=/dev/sdp  --whitelisted
[image: 计算机生成了可选文字:
司 ， SCSi id 
35000c500a29b17 （ 5 
-device-/dev/sdp 
- -whitelisted ]
 
vi /etc/udev/rules.d/99-woscore-sw-disks.rules
[image: 计算机生成了可选文字:
SYMLINK+z"WOSCOre 
SYMLINK+—"WOSCOre 
sd* ' 
SYMLINK+—"WOSCOre 
KERNEL—" Sd* " 
SYMLINK+—"WOSCOre 
sd* ' 
SYMLINK+z"WOSCOre 
SYMLINK+—"WOSCOre 
sd* ' 
sd* ' 
， 了 、 LI 卜 粼 + = " 、 VOS （ ore 
SYMLINK+—" 、 goscore 
sd* ' 
KERNEL—" S"" 丿 SUBSYSTEM——"blOCk" 
KERNEL—" Sd* " ， Sl 」 BSYSTEM——"blOCk" 
SUBSYSTEM——"b10ck" 
sd*' 丿 馴 B ， T 日 繼 b10 酞 “ 
KERNEL—" Sd* SUBSYSTEM——"blOCk" 
Sl 」 BSYSTEF 卜 —"block" 
9 」 B ST 繼 b10 醵 “ 
sd*' 丿 SUB ， T 日 繼 b10 酞 “ 
KERNEL—" Sd* SUBSYSTEM——"blOCk" 
KERNEL—" Sd* " ， Sl 」 BSYSTEM——"blOCk" 
9 」 B ST 繼 b10 醵 “ 
KERNEL—" Sd* SUBSYSTEM——"blOCk" 
KERNEL—" Sd* " ， Sl 」 BSYSTEM——"blOCk" 
9 」 B ST 繼 b10 醵 “ 
sd*' 丿 SUBS T 日 繼 b10 酞 “ 
馴 BS T 日 繼 b10 酞 PROGRAMÆ' /sbin/scsl id 
PRO( 1 = = “ /sbin/scsi id 
PROGRAM—" /sbin/scsi id --whitelisted 
F 0 M 一 “ /sbin/scsl id 
PROGRAMÆ' /sbin/scsl id 
PR 、 = = " /sbin/scsi id 
PROGRAM—" /sbin/scsl id --whitelisted 
PROGRAM—" /sbin/scsl id 
PRO 、 一 “ /sbin/scsl id 
PROGRAM—" /sbin/scsi id 
PRO 田 1 一 " /sbin/scsi id --whitelisted 
PROGRAM—" /sbin/scsl id 
PROGRAM—" /sbin/scsi id 
PROGRAM—" /sbin/scsi id --whitelisted 
PROGRAM—" /sbin/scsl id 
PROGRAM—"/sbin/SCS1 id 
--whitelisted 
--whltehsted 
--whltehsted 
--whitelisted 
--whltehsted 
--whltelusted 
--whitelisted 
--whltehsted 
--whltehsted 
--whitelisted 
--whltehsted 
--whltehsted 
- replace-whitespace 
- replace-whitespace 
replace-whitespace 
- replace-whitespace 
- replace-whitespace 
· replace-whitespace 
replace-whitespace 
- replace-whitespace 
- replace-whitespace 
· replace-whltespace 
replace-whitespace 
- replace-whitespace 
- replace-whltespace 
replace-whitespace 
-device 
z/dev/$name" 
-device 
-/dev/$name" 
-deuce 
-/dev/$name" 
-deuce 
Z/dev/$name" 
-device: 
/dev/$name" 
-device— 
/dev/$name" 
-deuce 
-/dev/$name" 
-deuce 
z/dev/$name" 
-device 
E/dev/$name" 
-device— 
/dev/$name" 
-deuce 
-/dev/$name" 
-deuce 
z/dev/$name" 
-device 
z/dev/$name" 
-device— 
/dev/$name" 
-deuce 
-/dev/$name" 
-deuce 
Z/dev/$name" 
RESULT—" 3 ， 儿 0c500a295B 厁 4 " 
RESULT—" 35000c 0a295 09 · 
3500 Oa2g5ae3b " 
3 ， 500a2g502f 
RES-ILT—" 3 ， 儿 0c500a295 59 · 
RES-LT—" 35000c500a296 d3d " 
35000c Oa2g5d 93 " 
RESULTz:" 3 ， 500a2g5e 酽 
RESULT—" 3 ， 0c500a295caf5 " 
RESULT—" 35000c500a29592e5 " 
35000c500a 凶 5bfeb " 
3 ， 500925agfg 酽 
RESULT—" 3 ， 儿 0c500a295B56 尹 
T—" 35000c500a295a314 " 
“ 35000c Oa2g6B7d 酽 
RE 
SY 、 L 巋 + 
， MLI 丨 巛 + 
SY 、 L 巋 + 
SYMLIFIK+Z" 
SY 、 L 巋 + 
， MLI 丨 + 
f 、 L + 
WO SC 0 re 
WO SC 0 re 
WO SC 0 re 
WO SC 0 re 
WO SC 0 re 
WO SC 0 re 
WO SC 0 re 
-disk01" 
-disk02" 
． di 酞 0 酽 
． di 酞 0 酽 
-disk05" 
-disk06" 
． di 07 " 
豳 i 酞 08 " 
-disk09" 
-disklO" 
． di 11 " 
． di 酞 12 " 
-disk13" 
-disk14" 
． di 酞 1 宁 
ATTRIqueue/scheduler)2"deadline" 
AITRIqueue/scheduler)-"deadline" 
ATTRIqueue/schedulerF"dead1ine' 
ATTRIqueue/scheduler)-"dead1ine 
ATTRIqueue/scheduler):"deadline" 
ATTRIqueue/scheduler)-"deadline" 
ATTRIqueue/scheduler)-"dead1ine' 
ATTRIqueue/scheduler)-"deadline' 
ATTRIqueue/scheduleN-"deadline" 
ATTRIqueue/scheduler)-"deadline" 
ATTRIqueue/scheduler)-"dead1ine' 
ATTRIqueue/scheduler)-"dead1ine' 
ATTRIqueue/scheduler)z"deadline" 
ATTRIqueue/scheduler)-"deadline" 
ATTRIqueue/scheduler)-"dead1ine' 
' ， SYMLIM(+z"woscore-disk16" 
ATTRIqueue/scheduler)-"deadline" ]
 
1. 重新启动udev
start_udev
 
1. 登录WOS后台查看状态是否为active
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root disk 15:15 /dev/sdb
root disk 15:14 /dev/sdc
root disk 15:14 /dev/sdd
root disk 15:15 /dev/sde
root disk 15:14 /dev/sdf
root disk 15:15 /dev/sdg
root disk 15:15 /dev/sdh
root disk 15:14 /dev/sdi
root disk 15:14 /dev/sdj
root disk 15:14 /dev/sdk
root disk 15:14 /dev/sdl
root disk 15:14 /dev/sdn
root disk 15:14 /dev/sdn
root disk 15:14 /dev/sdo
root disk 15:14 /dev/sdp
root disk 2019 /dev/sdq
root disk 2019 /dev/sdql
root disk 2019 /dev/sdq2

root disk

[root@swosda02-szzb ~]
20

[rooteswosdad2-szzb ~]# |

2019 /dev/sdq3
we -1




image6.png
[root@swosda02-szzb ~1# cat /etc/udev/rules.d/99-woscore-sw-disks.rules

“sd*", SUBSYSTEM=="block", “/sbin/scsi_id --whitelisted --replace-whitespace 35000¢50032958414" "woscore-disk0l", ATTR{queue/scheduler

"sd*", SUBSYSTEM=="block", "/shin/scsi_id --whitelisted --replace-whitespace dev/$name”, 35000¢500a2958a9" , SYMLINK+="woscore-disk02", ATTR{queue/scheduler:
"sd*", SUBSYSTEM=="block", /sbin/scsi_id --vhitelisted --replace-vhitespace =/dev/$nane” , 35000c500a295ae3b" , SYMLINK+="woscore-disk03*, ATTR{queue/scheduler}="
"sd*", SUBSYSTEM=="block", " /sbin/scsi_id --replace-whitespace dev/$name”, 35008¢500a29592fc” , SYMLINK+="woscore-diska4", ATTR{queue/scheduler}
"sd*", SUBSYSTEM=="block", " /sbin/scsi_id replace-hitespace dev/$name”, 350008¢500a2956059" , SYMLINK+="woscore-disk@5", ATTR{queue/scheduler:
"sd*", SUBSYSTEM=="block", " /sbin/scsi_id replace-vhi tespace dev/$name”, 35000¢500a2964d3d" , SYMLINK+="woscore-disk06", ATTR{queue/scheduler:
"sd*", SUBSYSTEM=="block", " /shin/scsi_id --replace-vhi tespace =/dev/§nane” , 350000500a2950493" , SYMLINK+="woscore-disk07*, ATTR{queue/scheduler}="
"sd*", SUBSYSTEM=="block", " /sbin/scsi_id --replace-whitespace dev/$name”, 35008¢500a295e6¢h” , SYMLINK+="woscore-disk@s", ATTR{queue/scheduler}
"sd*", SUBSYSTEM=="block", " /sbin/scsi_id replace-hitespace 350008¢500a295¢af5" , SYMLINK+="woscore-disk9", ATTR{queue/scheduler’
"sd*", SUBSYSTEM=="block", " /shin/scsi_id replace-vhi tespace 35000¢500a29592e5" , SYMLINK+="woscore-disk10", ATTR{queue/scheduler:
"sd*”, SUBSYSTEM=="block", " /shin/scsi_id --replace-vhi tespace 35000c500a295bfeb’, |, SYMLINK+="voscore-diskll", ATTRIqueue/scheduler}=
"sd*", SUBSYSTEM=="block", " /sbin/scsi_id --replace-whitespace 35008¢5 %%ﬂnsmm-duku”, ATTR{queue/scheduler}
"sd*", SUBSYSTEM=="block", " /sbin/scsi_id replace-whitespace 35000¢5 ? oscore-disk13", ATTR{queue/scheduler:
"sd*", SUBSYSTEM=="block", " /shin/scsi_id replace-vhitespace 35000¢500a295a314" Nk+="voscore-disk14", ATTR{queue/scheduler:
"sd*", SUBSYSTEM=="block", "/shin/scsi_id --whitelisted --replace-whitespace --device=/dev/$name”, " 350000500a29687d9" , SYML ‘woscore-disk15", ATTR{queue/scheduler}=
“sd*", SUBSYSTEM=="block", " fsbin/scsi_id --whitelisted --replace-whitespace --device=/dev/$name”, RESULT=="35000c508a29617¢5" , SYMLINK+="woscore-disk16", ATTR{queue/scheduler}="deadline"
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Lroot@swosda ~]# start_udev
Starting. udev:

Trooteswosdaoi-szzb ~1#
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~1# scsi_id --device=/dev/sdp --whitelisted

#1
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--device=/dev/§nane",
--device=/dev/§nane"
--device=/dev/§nane",
--device=/dev/¢name", RES|

--device=/dev/§nane”, RESULT=

" 35000c5003295841 4
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[root@swosda®2-szzb ~]# hdparm -I /dev/sdp

/dev/sdp:

ATA device, with non-removable media
tModel Number: ST
Serial Number:
Firmvare Revision
Transport:

Standards:
Used: unknown {minor revision code Gx006d)

Supported: 10987 65
Likely used: 10

PBAC

Serial, ATAB-AST, SATA 1.0a, SATA II Extensions, SATA Rev 2.5, SATA Rev 2.6, SATA Rev 3.0

Configuration:
Logical max current
cylinders 16333 16333

[CELEY 16 16
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t0 B8 o 10.0.1.238 shahe2 Active 182M 63958 51821 81
SlotID  « Status < Manufacturer < Model & Serial Number < Capacity ¢
1 Active AD1 ST4000NMOD35-1v4107 ZC11PBLA 4.00TB
2 Active AD2 ‘ST4000NM0O035-1V4107 ZC11PBMZ. 4.00T8
3 Active AD3 ST4000NMO035-1v4107 ZC11PEBO 4.00T8
4 Active AD4 ST4000NMO035-1v4107 ZC11NYRE 4.00T8
5 Active AD5 ST4000NMOD35-1v4107 ZC11PBJ3 4.00TB
6 Active ADB ‘ST4000NM0O035-1V4107 ZC11PAPOD 4.00T8
7 Active A07 ST4000NMO035-1v4107 ZC11PSX0 4.00T8
8 Active A08 ST4000NMO035-1v4107 ZC11PEX2 4.00T8
9 Active AD9 ST4000NMO035-1v4107 ZC1PSZ1 4.00TB
10 Active A10 ‘ST4000NM0O035-1V4107 ZC1LPY6 4.00T8
" Active AN ST4000NMO035-1v4107 ZC1PB1V 4.00T8
12 Active A12 ST4000NMOD35-1v4107 Zc1070CV 4.00T8
13 Active A13 ST4000NMOD35-1v4107 ZC11PBJH 4.00TB
14 Active Al4 ‘ST4000NM0O035-1V4107 ZC1NYR1 4.00T8
15 Active AlS ST4000NMO035-1v4107 ZC11PATS 4.00T8
16 Active Al6 ST4000NMO035-1v4107 l : I 4.00T8
Enclosure ID FAKE_ENCLOSURE
Software Version ¥2.7.0_1.0_g9cec8cd





