
按F2输入root密码
[image: ]

回车进入网络配置
[image: ]
回车进入IPV4 配置
[image: ]

空格选择静态ip配置
[image: ]

备注：ip配置好保存后如未生效，请检查网口是否启动。
[image: ]
空格启用后，重启网络服务后生效
[image: ]
Enable启用 shell和ssh服务
[image: ]
此时通过工具ssh远程登录无法输入秘钥，需要先按alt+f1进入shell终端修改ssh配置文件
/etc/ssh/sshd_config 
PasswordAuthentication yes
[image: ]

此时可通过xshell等工具输入密码正常远程
[image: ]
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Modify DCUI idle tineout

Modify the number of idle minutes that can elapse before you
nust log in again in DCUI.

Modify DCUI idle tineout

<Enter> Change
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running fron inetd
Port 2200

Protocol 2

HostKey /etc/ssh/ssh_host_rsa_key

# Fips node restricts ciphers to only FIPS-pernitted ciphers
Fipshode yes

# OpenSSH 7.8 suitched to af21/csl, which has been observed to cause
# connection drops. Override to earlier values.
1PQoS loudelay throughput

W uPP FCS_SSH_EXT.1.7: rekey after 168, 1H Cinstead of default 4GB for AES)
RekeyLinit 16, 1H

SyslogFacility auth
LogLevel info

PernitRootLogin yes

Printhotd yes
PrintLastLog no

TCPKeepAlive yes
X1iForuarding no

Ciphers aes256-gen@openssh. con, aes128-genBopenssh . con, aes256-ctr aes192-ctraes128-ctr
MACs hnac-sha2-256, hnac-sha2-512,hnac-shal

UsePAN yes

# only use PAN challenge-response (keyboard-interact ive)

PassuordAuthent icat ion yes

Banner /etc/issue

Subsysten sftp /usr/1ib/vauare/openssh/bin/sftp-server -f LOCALS -1 INFO

Author izedKeysF i le /etc/ssh/keys-7u/author ized_keys

# Tineout value of 10 mins. The default value of ClientAliveCountMax is 3.

# Hence, ue get a 3 = 200 = 600 seconds tineout i the client has been

# unrespons ive .

ClientAlivelnterval 200
[root@localhost

125 USERID

NUM
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* 1 lixinyuan.vip 2192.168.0.110:22 *

Type “help' to learn how to use Xshell prompt.
ssh 192.168.0.110

Connecting to 192.168.0.110:22...

Connection established.

To escape to local shell, press 'Ctrl+Alt+]'.
Connection closed by foreign host.

Disconnected from remote host(192.168.0.110:22) at 15:06:19.

Type “help' to learn how to use Xshell prompt.
ssh 192.168.0.110

Connecting to 192.168.0.110:22...
Connection established.
To escape to local shell, press 'Ctrl+Alt+]'.

Connection closed by foreign host.
Disconnected from remote host(192.168.0.110:22) at 15:10:56.
Type “help' to learn how to use Xshell prompt.

ssh 192.168.0.110

Connecting to 192.168.0.110:22...
Connection established.
To escape to local shell, press 'Ctrl+Alt+]'.

LN The remote SSH server rejected X11 forwarding request.
The time and date of this login have been sent to the system logs.

WARNING:
A1l commands run on the ESXi shell are logged and may be included in

support bundles. Do not provide passwords directly on the command line.

Most tools can prompt for secrets or accept them from standard input.

VMware offers supported, powerful system administration tools. Please
see www.vmware.com/go/sysadmintools for details.

The ESXi Shell can be disabled by an administrative user. See the

vSphere Security documentation for more information.
[root@localhost:~]

192.168.0.110:22,

SH2

xterm

™ 119x46
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Conf igure Managenent Netuork

Hostnane :
localhost

iConf igure Managenent Netuork IPu4 Address:
192.168.0.171

Netuork identity acquired from DHCP server 192.168.0.1

1Pu6 Addresses
fe80): :42f2:e9FF :fe26 abda/64

To vieu or modify this host’s managenent network settings in
detail, press <Enter>

<Enter> Hore <Esc> Log Out

VMuare ESXi 6.7.0 (VMKernel Release Build 14320388)
192.168.70125] | USERID | 3.0 tps | 0.999 KBis | Power ON
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1Pv4 Conf igurat ion

1Pv4 Conf igurat ion

This host can obtain an 1Pv4 address and other netuorking
paraneters autonatically if your network includes a DHCP
server. If not, ask your netuork adninistrator for the
appropriate settings.

<Enter> Change

VMuare ESXi 6.7.0 (VMKernel Release Build 14320388)
192.168.70125| | USERID || 1.6 ps | 1.202 KBIs | Power ON





image4.png
File View Macros Tools VirtualMedia Help

1Pu4 Configuration

This host can obtain netuork settings autonatically if your netuork
includes a DHCP server. If it does not. the follouing settings must be
specified:

Default Gateuay [ 192.168.0.1_

192.168.70.125| | USERID| | 4.0 fps || 0.32 KB num|| |5
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Netuork Adapters

Select the adapters for this host’s default managenent netuork

connection. Use tuo or more adapters for fault-tolerance and
load-balancing.

Intel 350 (...:e9:26:ab:da) Connected C

192.168.70.125| | USERID| | 2.0 fps || 2.642 KB

num|| |5
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Restart Managenent Netuork

Restart Managenent Netuork

Restarting the nanagenent network interface may be required
to restore netuorking or to renew a DHCP lease.

Restarting the managenent netuork will result in a brief
netuork outage that may tenporarily affect running virtual
nachines.

Note: If a reneued DHCP lease results in a new netuork
identity (e.g., IP address or hostnane), remote managenent
softuare uill be disconnected.

<Enter> Restart <Esc> Log Out
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